CONFIGURATION INFORMATION
=========================

Path         : /opt/ts32pl7/conf/instr/spect/uxnmr.info
Date         : Fri Jun 24 13:11:47 2022
Release      : TOPSPIN Version 3.2-pl7
Installed in : /opt/ts32pl7
Host         : rk700
OS           : CentOS release 5.8 (Final)
CPU          : Intel(R) Xeon(R) CPU W3505 @ 2.53GHz (2 cores at 1596 MHz)
User         : nmr (NMR User (nmr))
Description  : AVANCE III HD 700
Location     : International Tomography Center Novosibirsk
System       : Avance III NMR spectrometer
1H-frequency : 700.23 MHz
Order Number : 10068323
Configured in: /opt/ts32pl7/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.254
- Tctrl : 1
- Fctrls: 2
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU: AQS DRU-E Z102520/03061 ECL 07.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 150604
- DRU controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x53   0x5    CD  R  0.1 REC-1  AQS RXAD/2 1000 Z130589/26 ECL 00.01
     3   0x34 0xda   0x1        X  0.1 REF-1  
     4   0x24 0x33     0        S  2.4 SGU-1  AQS SGU/3 1200 (2CH) Z117130/00721 ECL 02.04 FPGA-Vs=20131031
    13   0xa0 0x93     0        V  0.0 PS-1   
    14   0xa1 0x91     0        V  1.1 PS-2   AQS PSM-D Power Supply Module
    --   0x20 0xd8     0        B  1.1 MASTER AQS/3+ Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345097_0234 W1345097/0234 ECL 20:
- TCP/IP address = 149.236.99.253
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H500/100/250 E 700-900MHZ INR: W1345097/0234 ECL 20
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/1568 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/6737 ECL 50
LTRX Z109891/00069 ECL 01.01:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 700: Z109891/00069 ECL 01.01

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20150423
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 700: Z109891/00069 ECL 01.01
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/01055 ECL 04.00
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/01229 ECL 01.03

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Preamplifiers :
HPPR: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Application firmware = c.
                no LED display for tuning and matching
    Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 100.0%/0.2deg, reflection meter)
                 PN=Z103206, SN=00092 from 20120831
    Module  2 : 2H
                 PN=Z003474, SN=00200 from 20120830
    Module  3 : XBB19F 2HS
                 PN=Z003507, SN=00660 from 20120830
    Module  4 : XBB19F 2HS
                 PN=Z003507, SN=00659 from 20120830
    Module  5 : 13C
                 PN=Z003525, SN=00147 from 20120823
    Module  6 : 15N
                 PN=Z003531, SN=00139 from 20120824


Frequency generation:
- F1: for SGU
- F2: for SGU



RF cable connections (detected by 'confamp')
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0234 at TCP/IP 149.236.99.253)
SGU1 AUX  output -> input 4 of transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0234 at TCP/IP 149.236.99.253)
SGU2 NORM output -> input 2 of transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0234 at TCP/IP 149.236.99.253)
SGU2 AUX  output -> TUNE signal input of HPPR

Blanking cable connections (detected by 'confamp')
--------------------------------------------------------------------
transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0234 at TCP/IP 149.236.99.253) amplifier 1H-100W uses blanking 2
transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0234 at TCP/IP 149.236.99.253) amplifier X-500W uses blanking 1
transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0234 at TCP/IP 149.236.99.253) amplifier 2H-250W uses blanking 3
transmitter 2 (BSMS/2 LOCK TRANSCEIVER 700 Z109891/00069 at TCP/IP 149.236.99.20) amplifier 2H-5W needs no blanking

